(footprint "TP4056-Module" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 61ECFE6F)
  (attr smd)
  (fp_text reference "REF**" (at 15.24 -12.7 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dd2f6b13-9e35-4a67-90ac-cf0d1ea34e5a)
  )
  (fp_text value "TP4056-Module" (at 15.24 -10.16 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3559e287-424e-4397-b080-77c7ba6f395b)
  )
  (fp_text user "B-" (at 23 -4 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 749dfe75-c0d6-4872-9330-29c5bbcb8ff8)
  )
  (fp_text user "IN-" (at 5.5 -1.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b635b16e-60bb-4b3e-9fc3-47d34eef8381)
  )
  (fp_text user "OUT-" (at 22 -1.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp da469d11-a8a4-414b-9449-d151eeaf4853)
  )
  (fp_text user "IN+" (at 5.5 -15.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dabe541b-b164-4180-97a4-5ca761b86800)
  )
  (fp_text user "OUT+" (at 22 -15.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dd00c2e1-6027-4717-b312-4fab3ee52002)
  )
  (fp_text user "B+" (at 23 -13 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fd470e95-4861-44fe-b1e4-6d8a7c66e144)
  )
  (fp_text user "${REFERENCE}" (at 15.24 -7.62 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp e6521bef-4109-48f7-8b88-4121b0468927)
  )
  (fp_line (start 0 -17.2) (end 0 0) (layer "F.SilkS") (width 0.12) (tstamp 57b46e54-0fd7-428f-89e9-2384adc40b64))
  (fp_line (start 28 -17.2) (end 28 0) (layer "F.SilkS") (width 0.12) (tstamp d250ce07-2cae-4efd-a4fd-02b1bd04a321))
  (fp_line (start 0 -17.2) (end 28 -17.2) (layer "F.SilkS") (width 0.12) (tstamp ef7ac9b1-db97-468d-83bd-7a544b867249))
  (fp_line (start 0 0) (end 28 0) (layer "F.SilkS") (width 0.12) (tstamp f7e200ad-0805-42f5-9f32-792f4044fcf7))
  (fp_line (start 0 0) (end 0 -17.2) (layer "F.CrtYd") (width 0.05) (tstamp 7e969d15-6cc0-4258-8b27-586608a21adb))
  (fp_line (start 28 -17.2) (end 28 0) (layer "F.CrtYd") (width 0.05) (tstamp 851ab59d-1fd7-45c7-a775-29797327cafc))
  (fp_line (start 0 -17.2) (end 28 -17.2) (layer "F.CrtYd") (width 0.05) (tstamp c5a1761e-3391-4e74-90c9-947fd66e1fc6))
  (fp_line (start 28 0) (end 0 0) (layer "F.CrtYd") (width 0.05) (tstamp edc9ab4f-487a-48dc-95f2-4d87f0e9cf9e))
  (fp_line (start 0 -12.2) (end -1 -12.2) (layer "F.Fab") (width 0.1) (tstamp a3668681-09b1-48f0-a7b1-f6b24183a469))
  (fp_line (start -1 -5.1) (end 0 -5.1) (layer "F.Fab") (width 0.1) (tstamp bbb15673-6d42-42b8-9d51-7515b3ad9ee9))
  (fp_line (start -1 -12.2) (end -1 -5.1) (layer "F.Fab") (width 0.1) (tstamp d0dfd7c1-401d-4f64-8463-f4c0813ac28f))
  (pad "1" thru_hole circle (at 2.5 -15.6) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp e83e0227-ac0f-4180-82bd-68d3a7b56476))
  (pad "2" thru_hole circle (at 2.5 -1.6) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 9a9f2d82-f64d-4264-8bec-c182528fc4de))
  (pad "3" thru_hole circle (at 25.5 -15.6) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 1b54105e-6590-4d26-a763-ecfcf81eedc4))
  (pad "4" thru_hole circle (at 25.5 -1.6) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 519f6e60-eb9c-479d-80df-fda781585c2a))
  (pad "5" thru_hole circle (at 25.5 -13.06) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 120a7b0f-ddfd-4447-85c1-35665465acdb))
  (pad "6" thru_hole circle (at 25.5 -4.14) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 23bb2798-d93a-4696-a962-c305c4298a0c))
)
