(module TP4056-18650 (layer F.Cu) (tedit 58E55FCB)
  (fp_text reference USB_CHRG** (at 13.6 19.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value TP4056-18650 (at 13 -1.6) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user "Battery Charger 1A" (at 12.7 8.9) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user GND (at 1.8 13.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user 5v (at 1.7 4.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 26.1 2.5) (end 26.1 15.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.1 15.4) (end 26.4 15.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.3 15.4) (end 28.4 15.4) (layer F.SilkS) (width 0.15))
  (fp_line (start 28.4 15.4) (end 28.4 15.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 26.3 0) (end 28.4 0) (layer F.SilkS) (width 0.15))
  (fp_line (start 28.4 0) (end 28.4 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 28.4 2.5) (end 26.1 2.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 28.4 15.7) (end 28.4 17.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 28.4 17.8) (end 0 17.8) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 17.8) (end 0 0) (layer F.SilkS) (width 0.15))
  (fp_text user B+ (at 21.7 5.1) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user B- (at 21.7 12.7) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Out+ (at 20.9 1.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user Out- (at 20.9 16.2) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user USB (at 1.6 9.1 90) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0.4 7.2) (end 2.9 7.2) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.9 7.2) (end 2.9 11) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.9 11) (end 0.4 11) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.4 11) (end 0.4 7.3) (layer F.SilkS) (width 0.15))
  (fp_text user - (at 4 16.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user + (at 3.9 1.6) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 0) (end 26.3 0) (layer F.SilkS) (width 0.15))
  (pad 6 thru_hole rect (at 24.6 12.8) (size 2.8 2.8) (drill 1.54) (layers *.Cu *.Mask))
  (pad 5 thru_hole rect (at 24.6 5.2) (size 2.8 2.8) (drill 1.54) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at 24.6 16.2) (size 2.8 2.8) (drill 1.54) (layers *.Cu *.Mask))
  (pad 3 thru_hole rect (at 24.6 1.7) (size 2.8 2.8) (drill 1.54) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 1.7 15.9) (size 2.8 2.8) (drill 1.54) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 1.7 1.7) (size 2.8 2.8) (drill 1.54) (layers *.Cu *.Mask))
)
